'Uge battle fORKtress to krush unlucky gitz not fast 'nuff to run away from this beast!

Print the larger parts with 0.12mm
Print the smaller parts with 0.1mm

As infill I used ca. 12% gyroid

The cab has two versions: with and without glyph to add your own if you want

No supports needed for:
- Fortress_Cab
- Fortress_DeffRolla_01
- Fortress_DeffRolla_Pin01
- Fortress_DeffRolla_Pin02
- Fortress_Engine_01
- Fortress_Hull_01
- Fortress_Hull_02
- Fortress_Hull_03
- Fortress_Hull_Top
- Fortress_Kannon02
- Fortress_Kannon03
- Fortress_Trakk01
- Fortress_Trakk02


Everything else (might) need regular supports
- Fortress_Engine_Exhaust prints best with tree support

Assembly:
- Please see the Pictures :-)
- Most parts will fit only where they should.
- Fortress_Cab_Beam01 & Fortress_Cab_Beam02 are holding the cab and belongs to Fortress_Hull_03, there are slight gaps where they fit (test without glue!)
- I recommend to paint first, then glue the parts since the interieur would be impossile to reach later.
- Fortress_Kannon01 has a slot or a 10x4mm magnet, glue this one in first and place it to the centre of the open or closed top. Then glue a 10x4mm magnet on the mating part (underside) for an easy removable kannon. Aso fits the Fortress_DeffRolla_Pins.
- The Fortress_Kannon02 (barrel) can bee glued on to fit the angle of open (high) or hard top (low) as in my pictures (design fits high angle, low doesn't fit perfect...but its not much visible later on...)
- The Fortress_Engine_01 is just glued centered to Fortress_Hull_02
- I did not glue the Fortress_Hull_Hard_Top, I wanted it to be removable.