                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


http://www.thingiverse.com/thing:2713364
Warhammer 40K Modular Trench by braeda is licensed under the Creative Commons - Attribution - Non-Commercial license.
http://creativecommons.org/licenses/by-nc/3.0/

# Summary

Added damaged blocked endpiece.
Added damaged straight piece.

Made for 28mm scale. 
Minor assembly after print.

The holes on the sides fits 3x2mm magnets, that are easily found worldwide.

# Print Settings

Printer Brand: Prusa
Printer: i3 MK2S
Rafts: No
Supports: No
Resolution: .2
Infill: 20%

# Post-Printing

## Step 1

Start assembly by gluing 2 magnets on one pice with negative on one side and positive on the other, and use something non magnetic to push them in properly. 

After that, take another two more magnets and put those on the 2 original magnets and add some superglue to them. Now take another piece and push it onto the 2 magnets and then slide the pieces apart sideways. 

Then do the same thing again but spin the piece around so that you have the magnets put in like in the picture below. 

Now you can use the piece with magnets on both sides as a guide in the same way as earlier and it will not matter which way the pieces are connected. 

They will always connect no matter how they are turned if this method is used!

![Alt text](https://cdn.thingiverse.com/assets/8b/5d/dd/be/b5/magnet_instructions.jpg)

## Step 2

After the magnets have been glued in place you can glue down meshpanels with superglue. Just use a few drops, and don't let it get on your fingers!