Due to some rescaling I needed to do in post, 
the scales of the various STEP files are not consistant. 
Here is the complete list of conversions:

*Note1: All STL files are correctly scaled and ready to print. 
	If at all possible, use the STL files.

*Note2: Some parts need to be mirrored. 
	This is to allow supportless printing as much as possible.
	Such items include, Drills, Blades, Lower Legs, Weapon sides, ect.  

*Note3: Pegs and slots are not included in the main body in order 
	to allow supportless printing. To assemble the main Body,
	simply line up the back edge of the model when gluing. 
	Instructions image #2.


STEP File Conversion:
Conversion:			Suggested Nozzle Size:
Quad gun parts 	-900%		0.4mm nozzle
Grav Flux parts -900%		0.2
Upper arm Joint	-1000%		0.4
Arm Joint	-900%		0.4
Drill arm parts -1000%		0.4
Claw arm parts	-1000%		0.4
80mm base	-1000%		0.4
Core 1		-1000%		0.4
Core 2		-1000%		0.4
Foot		-900%		0.4
Groin		-930%		0.2
Head		-1000%		0.2
Hips		-950%		0.4
Joint		-900%		0.4
Kneecap		-900%		0.2
Shoulder	-900%		0.4
Lower Leg	-900%		0.2
Side1,2		-1000%		0.4
missiles1,2	-1000%		0.2
Power Plamnt 	-1000%		0.2
Upper Leg	-900%		0.4